(Your Business Name Here) – Safe Work Procedure
DRILL SEEDER – TRACTOR OPERATED

DO NOT use this machine unless you have been instructed
in its safe use and operation and have been given permission

PERSONAL PROTECTIVE EQUIPMENT


[image: Foot protection must be worn]  	[image: Eye and hearing protection must be worn]		[image: Protective clothing must be worn]






PRE-OPERATIONAL SAFETY CHECKS
Locate and ensure you are familiar with all machine operations and controls. 
Operate only with roll over protection structure (ROPS) and seatbelt equipped tractors.
[bookmark: OLE_LINK14][bookmark: OLE_LINK15][bookmark: OLE_LINK24][bookmark: OLE_LINK25][bookmark: OLE_LINK16][bookmark: OLE_LINK17]Ensure all guards are fitted, secure and functional. Do not operate if guards are missing or faulty.
Ensure the 3 point linkage, securing pinions and safety chains are in sound condition.
Ensure the rotary slasher is attached according to manufacturer’s specification.
Ensure the hopper lid is locked or interlocked and the interlocking device (if fitted) is functioning.
Check the tyre pressure on the drill seeder and tractor.
Ensure the PTO and driveline guard are functioning.
Ensure the hydraulic rams, hoses and couplings are in sound condition.

OPERATIONAL SAFETY CHECKS
Keep clear of moving machine parts.
Ensure the seed metering mechanism is functioning and in sound condition.
Ensure the towing mechanism, securing pinions and safety chains are in sound condition.
Ensure the coulters are in sound condition.
Ensure the power source to the hopper is disengaged before opening the lid.
Ensure the hopper lid is locked after topping up with seed.
Ensure no person or animal is endangered when operating equipment.

ENDING OPERATIONS AND CLEANING UP
Remove any foreign material from in and around coulters, spacers and hydraulic rams.
Keep the work area and implement shed in a safe, clean and tidy condition.

POTENTIAL HAZARDS AND INJURIES
Moving parts.
Noise.
[bookmark: OLE_LINK8][bookmark: OLE_LINK9][bookmark: OLE_LINK13]Hair/clothing getting caught in moving machine parts.
[bookmark: OLE_LINK4][bookmark: OLE_LINK5]
DON’T
Do not use faulty equipment.  Report suspect machinery immediately.



























This safe work procedure does not necessarily cover all possible hazards associated with this equipment and should be used in conjunction with other references. 
It is designed as a guide to be used to compliment training and as a reminder to users prior to equipment use.

ALWAYS refer to the manufacturer’s instructions when writing your own safe work procedure.
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