(Your Business Name Here) – Safe Work Procedure
POWER BLOWER – PETROL OPERATED

DO NOT use this machine unless you have been instructed
in its safe use and operation and have been given permission

PERSONAL PROTECTIVE EQUIPMENT
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PRE-OPERATIONAL SAFETY CHECKS
Locate and ensure you are familiar with all machine operations and controls.
Check for loose/missing nuts, bolts and screws. Tighten and/or replace as needed.
Inspect fuel lines, tank and area around carburetor for fuel leaks. Do not operate if leaks are found.
[bookmark: OLE_LINK14][bookmark: OLE_LINK15][bookmark: OLE_LINK24][bookmark: OLE_LINK25][bookmark: OLE_LINK16][bookmark: OLE_LINK17]Ensure all guards are fitted, secure and functional. Do not operate if guards are missing or faulty.

OPERATIONAL SAFETY CHECKS
Ensure that no person or animal is endangered when operating equipment.
When starting, stand the machine upright on a level surface. Check that blower pipe is not blocked by the ground or by any objects.
Allow the machine to warm up at fast idle for a few minutes before using.
Keep a firm grip. Hold handle with fingers together encircling handle.
Maintain a straight wrist position. Avoid using your wrist in a bent, extended or twisted position.
Make sure the muffler side of the engine is away from your body to avoid burns.
Maintain a proper balance and secure footing. Do not work on slippery, uneven or unstable surfaces. Do not work in odd positions or on ladders.
Take wind conditions into account. Avoid open doors and windows.
Minimise dust by using blower at lower speeds. 
Always keep exhaust area clear of flammable debris.
Disconnect spark plug wire before you work on the unit or leave it unattended.
Allow the engine and muffler to completely cool before refuelling or performing any maintenance work.


ENDING OPERATIONS AND CLEANING UP
Remove any foreign material from in and around engine, air intake and guards.
Keep the work area and implement shed in a safe,  clean and tidy condition.

POTENTIAL HAZARDS AND INJURIES
Noise.
Flying debris.
Dust.
Vibration.
Burns from exhaust.

DON’T
[bookmark: OLE_LINK4][bookmark: OLE_LINK5]Do not use faulty equipment.  Report suspect machinery immediately.
Do not use any attachment or accessory unless it is recommended in the operator's manual.
Do not direct the blower towards other people.
Never use a higher speed setting then necessary to perform a task. 















This safe work procedure does not necessarily cover all possible hazards associated with this equipment and should be used in conjunction with other references. 
It is designed as a guide to be used to compliment training and as a reminder to users prior to equipment use.

ALWAYS refer to the manufacturer’s instructions when writing your own safe work procedure.
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