(Your Business Name Here) – Safe Work Procedure
ROTARY SLASHER – TRACTOR OPERATED

DO NOT use this machine unless you have been instructed
in its safe use and operation and have been given permission

PERSONAL PROTECTIVE EQUIPMENT


[image: PERSONAL PROTECTIVE EQUIPMENT SIGN - FOOT PROTECTION MUST BE WORN]  	[image: PERSONAL PROTECTIVE EQUIPMENT SIGN - EYE & HEARING PROTECTION MUST BE WORN]		[image: PERSONAL PROTECTIVE EQUIPMENT SIGN - PROTECTIVE CLOTHING MUST BE WORN]




PRE-OPERATIONAL SAFETY CHECKS
[bookmark: OLE_LINK10][bookmark: OLE_LINK11][bookmark: OLE_LINK19][bookmark: OLE_LINK20]Locate and ensure you are familiar with all machine operations and controls.
Operate only with roll over protection structure (ROPS) and seatbelt equipped tractors.
[bookmark: OLE_LINK14][bookmark: OLE_LINK15][bookmark: OLE_LINK24][bookmark: OLE_LINK25][bookmark: OLE_LINK16][bookmark: OLE_LINK17]Ensure all guards are fitted, secure and functional. Do not operate if guards are missing or faulty.
Ensure the 3 point linkage, securing pinions and safety chains are in sound condition.
Ensure the blades and fasteners are in sound condition.
Ensure the hydraulic rams, hoses and couplings are in sound condition.
Ensure the rotary slasher is attached according to manufacturer’s specification.

OPERATIONAL SAFETY CHECKS 
Keep clear of moving machine parts.
Be sure the transmission is out of gear and the mower blade clutch disengaged before starting the engine.
Ensure moving parts have stopped completely before doing any repair work.
Securely support the slasher before working underneath. Chock tractor wheels.
Lock up raised wings (where fitted) before transporting.

ENDING OPERATIONS AND CLEANING UP
Before dismounting the tractor:
· Lower rotary cutter to ground and allow moving parts to stop.
· Stop engine and set brake. 
· Remove key.
Remove any foreign material from in and around blades, fasteners, guards and hydraulic rams.
Keep the work area and implement shed in a safe, clean and tidy condition.


POTENTIAL HAZARDS AND INJURIES
Rapidly rotating blades.
Eye injuries.
Flying debris.
Noise.

[bookmark: OLE_LINK4][bookmark: OLE_LINK5]DON’T
Do not use faulty equipment.  Report suspect machinery immediately.
Do not allow passengers on the tractor or rotary slasher.
Do not use with anyone in area.
Do not cut with raised wings (where fitted) in raised or transport position.






















This safe work procedure does not necessarily cover all possible hazards associated with this equipment and should be used in conjunction with other references. 
It is designed as a guide to be used to compliment training and as a reminder to users prior to equipment use.

ALWAYS refer to the manufacturer’s instructions when writing your own safe work procedure.
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